configfile: "config.yaml"
include: "../rules/common.smk"
include: "../rules/renv.smk"
include: "../rules/preprocessing.smk"
include: "../rules/features.smk"
include: "../rules/reports.smk"

import itertools

files_to_compute = []

if len(config["PIDS"]) == 0:
    raise ValueError("Add participants IDs to PIDS in config.yaml. Remember to create their participant files in data/external")

if config["PHONE_VALID_SENSED_BINS"]["COMPUTE"] or config["PHONE_VALID_SENSED_DAYS"]["COMPUTE"]: # valid sensed bins is necessary for sensed days, so we add these files anyways if sensed days are requested
    if len(config["PHONE_VALID_SENSED_BINS"]["PHONE_SENSORS"]) == 0:
            raise ValueError("If you want to compute PHONE_VALID_SENSED_BINS or PHONE_VALID_SENSED_DAYS, you need to add at least one PHONE_SENSOR to [PHONE_VALID_SENSED_BINS][PHONE_SENSORS] in config.yaml")

    files_to_compute.extend(expand("data/raw/{pid}/{sensor}_raw.csv", pid=config["PIDS"], sensor=map(str.lower, config["PHONE_VALID_SENSED_BINS"]["PHONE_SENSORS"])))
    files_to_compute.extend(expand("data/raw/{pid}/{sensor}_with_datetime.csv", pid=config["PIDS"], sensor=map(str.lower, config["PHONE_VALID_SENSED_BINS"]["PHONE_SENSORS"])))
    files_to_compute.extend(expand("data/interim/{pid}/phone_sensed_bins.csv", pid=config["PIDS"]))
    files_to_compute.extend(expand("data/interim/{pid}/phone_sensed_timestamps.csv", pid=config["PIDS"]))

if config["PHONE_VALID_SENSED_DAYS"]["COMPUTE"]:
    files_to_compute.extend(expand("data/interim/{pid}/phone_valid_sensed_days_{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins.csv",
                                pid=config["PIDS"],
                                min_valid_hours_per_day=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_HOURS_PER_DAY"],
                                min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))

for provider in config["PHONE_MESSAGES"]["PROVIDERS"].keys():
    if config["PHONE_MESSAGES"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_messages_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_messages_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_messages_features/phone_messages_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_MESSAGES"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_messages.csv", pid=config["PIDS"]))

for provider in config["PHONE_CALLS"]["PROVIDERS"].keys():
    if config["PHONE_CALLS"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_calls_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_calls_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_calls_with_datetime_unified.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_calls_features/phone_calls_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_CALLS"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_calls.csv", pid=config["PIDS"]))

for provider in config["PHONE_BLUETOOTH"]["PROVIDERS"].keys():
    if config["PHONE_BLUETOOTH"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_bluetooth_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_bluetooth_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_bluetooth_features/phone_bluetooth_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_BLUETOOTH"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_bluetooth.csv", pid=config["PIDS"]))

for provider in config["PHONE_ACTIVITY_RECOGNITION"]["PROVIDERS"].keys():
    if config["PHONE_ACTIVITY_RECOGNITION"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_activity_recognition_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_activity_recognition_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_activity_recognition_with_datetime_unified.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_activity_recognition_episodes.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_activity_recognition_episodes_resampled.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_activity_recognition_episodes_resampled_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_activity_recognition_features/phone_activity_recognition_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_ACTIVITY_RECOGNITION"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_activity_recognition.csv", pid=config["PIDS"]))


for provider in config["PHONE_BATTERY"]["PROVIDERS"].keys():
    if config["PHONE_BATTERY"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_battery_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_battery_episodes.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_battery_episodes_resampled.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_battery_episodes_resampled_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_battery_features/phone_battery_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_BATTERY"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_battery.csv", pid=config["PIDS"]))


for provider in config["PHONE_SCREEN"]["PROVIDERS"].keys():
    if config["PHONE_SCREEN"]["PROVIDERS"][provider]["COMPUTE"]:
        if "PHONE_SCREEN" in config["PHONE_VALID_SENSED_BINS"]["PHONE_SENSORS"]:
            files_to_compute.extend(expand("data/interim/{pid}/phone_sensed_bins.csv", pid=config["PIDS"]))
        else:
            raise ValueError("Error: Add PHONE_SCREEN (and as many phone sensor as you have in your database) to [PHONE_VALID_SENSED_BINS][PHONE_SENSORS] in config.yaml. This is necessary to compute phone_sensed_bins (bins of time when the smartphone was sensing data)")
        files_to_compute.extend(expand("data/raw/{pid}/phone_screen_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_screen_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_screen_with_datetime_unified.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_screen_episodes.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_screen_episodes_resampled.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_screen_episodes_resampled_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_screen_features/phone_screen_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_SCREEN"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_screen.csv", pid=config["PIDS"]))

for provider in config["PHONE_LIGHT"]["PROVIDERS"].keys():
    if config["PHONE_LIGHT"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_light_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_light_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_light_features/phone_light_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_LIGHT"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_light.csv", pid=config["PIDS"],))

for provider in config["PHONE_ACCELEROMETER"]["PROVIDERS"].keys():
    if config["PHONE_ACCELEROMETER"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_accelerometer_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_accelerometer_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_accelerometer_features/phone_accelerometer_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_ACCELEROMETER"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_accelerometer.csv", pid=config["PIDS"]))

for provider in config["PHONE_APPLICATIONS_FOREGROUND"]["PROVIDERS"].keys():
    if config["PHONE_APPLICATIONS_FOREGROUND"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_applications_foreground_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_applications_foreground_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_applications_foreground_with_datetime_with_categories.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_applications_foreground_features/phone_applications_foreground_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_APPLICATIONS_FOREGROUND"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_applications_foreground.csv", pid=config["PIDS"]))

for provider in config["PHONE_WIFI_VISIBLE"]["PROVIDERS"].keys():
    if config["PHONE_WIFI_VISIBLE"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_wifi_visible_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_wifi_visible_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_wifi_visible_features/phone_wifi_visible_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_WIFI_VISIBLE"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_wifi_visible.csv", pid=config["PIDS"]))

for provider in config["PHONE_WIFI_CONNECTED"]["PROVIDERS"].keys():
    if config["PHONE_WIFI_CONNECTED"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_wifi_connected_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_wifi_connected_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_wifi_connected_features/phone_wifi_connected_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_WIFI_CONNECTED"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_wifi_connected.csv", pid=config["PIDS"]))

for provider in config["PHONE_CONVERSATION"]["PROVIDERS"].keys():    
    if config["PHONE_CONVERSATION"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/phone_conversation_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_conversation_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/raw/{pid}/phone_conversation_with_datetime_unified.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_conversation_features/phone_conversation_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_CONVERSATION"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_conversation.csv", pid=config["PIDS"]))

for provider in config["PHONE_LOCATIONS"]["PROVIDERS"].keys():
    if config["PHONE_LOCATIONS"]["PROVIDERS"][provider]["COMPUTE"]:
        if config["PHONE_LOCATIONS"]["LOCATIONS_TO_USE"] == "RESAMPLE_FUSED":
            if "PHONE_LOCATIONS" in config["PHONE_VALID_SENSED_BINS"]["PHONE_SENSORS"]:
                files_to_compute.extend(expand("data/interim/{pid}/phone_sensed_bins.csv", pid=config["PIDS"]))
            else:
                raise ValueError("Error: Add PHONE_LOCATIONS (and as many PHONE_SENSORS as you have) to [PHONE_VALID_SENSED_BINS][PHONE_SENSORS] in config.yaml. This is necessary to compute phone_sensed_bins (bins of time when the smartphone was sensing data) which is used to resample fused location data (RESAMPLED_FUSED)")

        files_to_compute.extend(expand("data/raw/{pid}/phone_locations_raw.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_locations_processed.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_locations_processed_with_datetime.csv", pid=config["PIDS"]))
        files_to_compute.extend(expand("data/interim/{pid}/phone_locations_features/phone_locations_{language}_{provider_key}.csv", pid=config["PIDS"], language=config["PHONE_LOCATIONS"]["PROVIDERS"][provider]["SRC_LANGUAGE"].lower(), provider_key=provider.lower()))
        files_to_compute.extend(expand("data/processed/features/{pid}/phone_locations.csv", pid=config["PIDS"]))

if config["FITBIT_HEARTRATE"]["TABLE_FORMAT"] not in ["JSON", "CSV"]:
    raise ValueError("config['FITBIT_HEARTRATE']['TABLE_FORMAT'] should be JSON or CSV but you typed" + config["FITBIT_HEARTRATE"]["TABLE_FORMAT"])

if config["FITBIT_STEPS"]["TABLE_FORMAT"] not in ["JSON", "CSV"]:
    raise ValueError("config['FITBIT_STEPS']['TABLE_FORMAT'] should be JSON or CSV but you typed" + config["FITBIT_STEPS"]["TABLE_FORMAT"])

if config["FITBIT_CALORIES"]["TABLE_FORMAT"] not in ["JSON", "CSV"]:
    raise ValueError("config['FITBIT_CALORIES']['TABLE_FORMAT'] should be JSON or CSV but you typed" + config["FITBIT_CALORIES"]["TABLE_FORMAT"])

if config["FITBIT_SLEEP"]["TABLE_FORMAT"] not in ["JSON", "CSV"]:
    raise ValueError("config['FITBIT_SLEEP']['TABLE_FORMAT'] should be JSON or CSV but you typed" + config["FITBIT_SLEEP"]["TABLE_FORMAT"])

for provider in config["FITBIT_HEARTRATE"]["PROVIDERS"].keys():
    if config["FITBIT_HEARTRATE"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_heartrate_{fitbit_data_type}_raw.csv", pid=config["PIDS"], fitbit_data_type=(["json"] if config["FITBIT_HEARTRATE"]["TABLE_FORMAT"] == "JSON" else ["summary", "intraday"])))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_heartrate_{fitbit_data_type}_parsed.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_heartrate_{fitbit_data_type}_parsed_with_datetime.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))

for provider in config["FITBIT_STEPS"]["PROVIDERS"].keys():
    if config["FITBIT_STEPS"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_steps_{fitbit_data_type}_raw.csv", pid=config["PIDS"], fitbit_data_type=(["json"] if config["FITBIT_STEPS"]["TABLE_FORMAT"] == "JSON" else ["summary", "intraday"])))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_steps_{fitbit_data_type}_parsed.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_steps_{fitbit_data_type}_parsed_with_datetime.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))

for provider in config["FITBIT_CALORIES"]["PROVIDERS"].keys():
    if config["FITBIT_CALORIES"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_calories_{fitbit_data_type}_raw.csv", pid=config["PIDS"], fitbit_data_type=(["json"] if config["FITBIT_CALORIES"]["TABLE_FORMAT"] == "JSON" else ["summary", "intraday"])))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_calories_{fitbit_data_type}_parsed.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_calories_{fitbit_data_type}_parsed_with_datetime.csv", pid=config["PIDS"], fitbit_data_type=["summary", "intraday"]))

for provider in config["FITBIT_SLEEP"]["PROVIDERS"].keys():
    if config["FITBIT_SLEEP"]["PROVIDERS"][provider]["COMPUTE"]:
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_sleep_{fitbit_data_type}_raw.csv", pid=config["PIDS"], fitbit_data_type=(["json"] if config["FITBIT_SLEEP"]["TABLE_FORMAT"] == "JSON" else ["summary", "intraday"])))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_sleep_{fitbit_data_type}_parsed_episodes.csv", pid=config["PIDS"], fitbit_data_type=["summary"]))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_sleep_{fitbit_data_type}_parsed.csv", pid=config["PIDS"], fitbit_data_type=["intraday"]))
        files_to_compute.extend(expand("data/raw/{pid}/fitbit_sleep_{fitbit_data_type}_parsed_with_datetime.csv", pid=config["PIDS"], fitbit_data_type=["intraday"]))

# visualization for data exploration
if config["HEATMAP_FEATURES_CORRELATIONS"]["PLOT"]:
    files_to_compute.extend(expand("reports/data_exploration/{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins/heatmap_features_correlations.html", min_valid_hours_per_day=config["HEATMAP_FEATURES_CORRELATIONS"]["MIN_VALID_HOURS_PER_DAY"], min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))
    
if config["HISTOGRAM_VALID_SENSED_HOURS"]["PLOT"]:
    files_to_compute.extend(expand("reports/data_exploration/{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins/histogram_valid_sensed_hours.html", min_valid_hours_per_day=config["HISTOGRAM_VALID_SENSED_HOURS"]["MIN_VALID_HOURS_PER_DAY"], min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))

if config["HEATMAP_DAYS_BY_SENSORS"]["PLOT"]:
    files_to_compute.extend(expand("reports/interim/{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins/{pid}/heatmap_days_by_sensors.html", pid=config["PIDS"], min_valid_hours_per_day=config["HEATMAP_DAYS_BY_SENSORS"]["MIN_VALID_HOURS_PER_DAY"], min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))
    files_to_compute.extend(expand("reports/data_exploration/{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins/heatmap_days_by_sensors_all_participants.html", min_valid_hours_per_day=config["HEATMAP_DAYS_BY_SENSORS"]["MIN_VALID_HOURS_PER_DAY"], min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))

if config["HEATMAP_SENSED_BINS"]["PLOT"]:
    files_to_compute.extend(expand("reports/interim/heatmap_sensed_bins/{pid}/heatmap_sensed_bins.html", pid=config["PIDS"]))
    files_to_compute.extend(["reports/data_exploration/heatmap_sensed_bins_all_participants.html"])

if config["OVERALL_COMPLIANCE_HEATMAP"]["PLOT"]:
    files_to_compute.extend(expand("reports/data_exploration/{min_valid_hours_per_day}hours_{min_valid_bins_per_hour}bins/overall_compliance_heatmap.html", min_valid_hours_per_day=config["OVERALL_COMPLIANCE_HEATMAP"]["MIN_VALID_HOURS_PER_DAY"], min_valid_bins_per_hour=config["PHONE_VALID_SENSED_DAYS"]["MIN_VALID_BINS_PER_HOUR"]))


rule all:
    input:
        files_to_compute

rule clean:
    shell:
        "rm -rf data/raw/* && rm -rf data/interim/* && rm -rf data/processed/* && rm -rf reports/figures/* && rm -rf reports/*.zip && rm -rf reports/compliance/*"